**IFC TAG modification 105.6.4**

**1. State Building Code to be Amended:**

 [ ]  International Building Code [ ]  State Energy Code

 [ ]  ICC ANSI A117.1 Accessibility Code [ ]  International Mechanical Code

 [ ]  International Existing Building Code [ ]  International Fuel Gas Code

 [ ]  International Residential Code [ ]  NFPA 54 National Fuel Gas Code

 [x]  International Fire Code [ ]  NFPA 58 Liquefied Petroleum Gas Code

 [ ]  Uniform Plumbing Code [ ]  Wildland Urban Interface Code

 **Section(s): IFC 105.6.4 and IFC 5307.1**

 **Title: Carbon dioxide systems ~~used in beverage dispensing applications~~.**

**2. Proponent Name (Specific local government, organization or individual): see below**

**3. Designated Contact Person:**

 **Name: Traci Harvey**

 **Title: Fire Protection Engineer**

 **Address: 2120 N. Wilbur, Spokane Valley, WA 99206**

 **Office Phone: (509) 892-4183**

 **Cell: (509) 496-4345**

 **E-Mail address: harveyt@spokanevalleyfire.com**

**4. Proposed Code Amendment**. Reproduce the section to be amended by underlining all added language, striking through all deleted language. Insert new sections in the appropriate place in the code in order to continue the established numbering system of the code. If more than one section is proposed for amendment or more than one page is needed for reproducing the affected section of the code additional pages may be attached. (Examples on the SBCC [website](https://fortress.wa.gov/ga/apps/sbcc/Page.aspx?nid=191))

 **Code(s)** International Fire Code **Section(s)** 105.6.4 and 5307.1 (Revised)

 105.6.4 Carbon dioxide systems ~~used in beverage dispensing applications~~. An operational permit is required for carbon dioxide systems ~~used in beverage dispensing applications~~ having more than 100 pounds of carbon dioxide.

5307.1 General. Carbon dioxide systems with more than 100 pounds (45.4kg) of carbon dioxide ~~used in beverage dispensing applications~~ shall comply with Sections 5307.2 through 5307.5.2.